

* **Motor Options:**

-Lithium Ion

-Conventional Battery: charged via outlet or solar power

-12V DC: low voltage, plug-in

-120V AC: plug in or hardwired

* **Control Options:**

-Mobile App

-Remote: 1 and 15 channels

-Wall Switch: 5 channels, simple wall surface installation

-Rooted Wall Switch: 1, 2 and 5 channels, Requires cutting into drywall.

* **Ideal for both Residential and Commercial projects:**

-Simple installation & operation

-Intergratable into existing automation systems

-Customizable limits and settings

-Retrofit brackets with Skyline and R-Series systems

-Multiple finishing options of Fascia and Cassette 